1) Install the Flex Control Builder (FCB).  The FCB installer can be found in the Firmware & Software tab of the website link under either Flex Control Systems or 6" Table Box w/ FLEX Control.

2) Get Library Files in FCB by opening FCB, clicking on the “Update & About” button and then the “Get Library Files” button. Click “Close” when complete and exit FCB.

3) Install Flex IO-16 Builder, available as one of resources in the .zip.

4) To keep library files obtained in step 2 up to date, repeat step 2.