Explaination of the TIE LINE

When the tie line cable is connected between two or more ML-116 systems, the audio in a room or combined group from one system can be fed to another room or combined group in another system.  This feature would permit audio monitoring (listen in) capability of one system by another.  A typical application of this feature would be a “green room” (waiting) situation or a prefunction area.

The TIE LINE function is controlled via the FM PANEL software. The TIE LINE  options menu is accessable from the ML116 FM PANEL toolbar.  Click on “TIE LINE” to assign source and destination selections.  Any rooms or groups selected for tieline operation will turn yellow.  The source room or group will be flagged with an “S” and the Destination room or group will be flagged with a “D”. 

Example:

ML116 System #1 has a room or combined group active.  There is a “green room” on the ML116 system #2 where the audio from System #1 needs to be fed and monitored.  The user would select System #1’s room or group as the “source and system 2’s room or group as the destination.  Audio is now “piped into the destination room(s) in group #2.

