Using the Touch MAP/Monitor Panel.

The Touch MAP/Monitor Panel acts as a master control point. It will display the Facility layout map graphic user interface and provide full room control and adjustment.  It will also display  room 

status and audio levels by emulating individual wallplate functions and status indicators.

To combine (mix) rooms:

Touch each room box once in the group you wish to combine.  A popup will ask for confirmation and display the room numbers you have selected to group. After touching yes the combined rooms will be shaded the same color and combined.

To break up a combined group:

Touch any of the combined rooms boxes once.  A popup will ask for confirmation.  Touch the “Break Group” option to un-combine.  The shading on the un-combined group will disappear.

To remove individual rooms from a group:

This function is only useable when three or more rooms are combined in a group.

Touch on the shaded group.  The edges of the grouped room boxes will highlight and a window will appear.    Select “Remove Room”.  A pulldown menu will appear with the all the room names in that group.  Select the name of the room to break and touch “OK.”  The room will loose its shading and operate independently while leaving the remaining rooms combined.
To call up a wallplate for control or status:

Double touch on the desired room box.  The graphic for that rooms' wall plate will  appear and show that rooms current status just as if you were standing at the actual wallplate. Audio will be active at the local speaker at this time and the 'listen in" feature is enabled.  Simply make the desired adjustments via touch and exit by touching main menu pick box. Details on the individual control adjustments are detailed in chapter 3.

Options Menu: 

Touch the "OPTIONS" pick box to open the options menu.  There are three option choices:

Screen Saver Settings-  Turns screen saver feature on or off. 

 Sets the time period before screen saver becomes active.



Monitor External Zones-  Selects and drives two auxilliary relays on the Monitor relay card 

and enables “listen in”  capability for one of two auxilliary zones 

through the monitor speaker.

Security Settings-  Allows one time user password change after each power up. 

Selects lockout device preference of Touch Map/Monitor panel and or remote wallplate  lockout.

Sets delay before lockout time period. 

NOTE:   The current saved password must be entered before a new password can be selected.

 If a password is lost or forgotten it can only be cleared and reset by the following 

procedure:

Power the system down.  Slide the CPU card out and close dip switch 13.  Slide the CPU

 card back in and power up to clear the password.  Power down again and set dip switch

 back to the original open position.  A new password can now be entered via the Touch MAP/Monitor Panel. 

